#Global delay (ms) between send command and receive answer:
globaldelay:300
6C FE F1 20
6C FE F1 28 00

#Loop 4 cycles:
loop:4 
8c fe f0 3f
endloop

#Create variable, name: var1, size 3 bytes, value 0C
variable:var1:3:0C
loop:10
#Replace var1 by value of var1(first cycle: 00 00 0C)
6c 10 f0 35 00 10 00 var1
#Increment variable every cycle by A0:
variable:var1:3:+A0
endloop

#setvariable:name:size:position
#Send command and set variable from response bytes:
setvariable:myvarX:3:4
6C 10 F0 3C 0A


#Add delay (milliseconds)
delay:100

#Add delay (milliseconds)
t:100

#getseed:startbyte:algo
#For unlocking, row1:settings for get seed command, row2: command to get seed, row3: unlock command
getseed:5:5b
6c 10 f0 27 01
6c 10 f0 27 02 key


loop:10
#break loop if byte 3 == 3C
break:3:3C
6C 10 F0 3C 0A
endloop

loop:10
#break loop if byte 2 != 3C
break!:2:3C
6C 10 F0 3C 0A
endloop

#Add block checksum:
6C 10 F0 36 00 00 FF 04 7C 7F 44 60 0A 7A 01 11 C5 91 5D 11 C5 blchk:2:1500
